Pre start checks:

1) Avionics OFF Check/SET
2) Gen1 and Gen2 OFF Check/SET
3) "Feathering Lever to "Fuel cutoff" (pull!) Check/SET
4) Throttle IDLE Check/SET

Cold Start Sequence:

a) Battery ON
b) Engine Ignition ON
c) At ITT of about 14% Set Condition Lever to Ground Idle (the engine is STARTED!)
d) Gen 1 ON
e) Gen 2 ON
f) Avionics ON

Ready to Taxi!

Note if you want to use the FS GPS in place of the Bendix/King, you will have to
modify the panel cfg. rename panel.cfg to bk_panel.cfg and then rename the 
fsgps_panel.cfg to panel.cfg and your all set.
