IMPORTANT - PLEASE READ!! for PAD D0228 FSX

To install simply copy the texture folder in your PAD D0228 folder. 

NB Make sure you are using an aircraft with the do2282_gmar13.mdl model file or later or the textures may not show properly.

Then copy and paste the text from here to the PAD D0228 Aircraft.cfg 


You will have to manually copy and paste this data into your aircraft.cfg file in order for this new
livery to show up in the simulator.

Step 1. Copy all of the data show below the dotted line.
Step 2. Open your aircraft.cfg file located in your PAD D0228 folder in the FSX\Aircraft\PAD D0228xxxxx\ directory.
Step 3. Paste the date after the last entry for aircraft. IE - [fltsim.xx] (xx = the entry value)
Step 4. Save your changes and close your file. Start the sim and select your livery from the list. Enjoy!!
------------------------------------------------

[fltsim.xx]
title=do228_212_Tradewind Alaska
sim=do228
model=
panel=dornier228x
sound=0
texture=ta
kb_checklists=do228_check
kb_reference=do228_ref
atc_id=N228TA
atc_airline=Tradewinds
ui_manufacturer=Dornier
ui_type=Do 228
ui_variation=Dornier 228-212 Tradewind Alaska
ui_typerole="Twin Engine TurboProp"
ui_createdby="PAD"
description=Dornier 228-212 19 seat STOL feeder liner & freighter.\nLength: 54.3 ft\nSpan: 55.7 ft\n Engines: 2 Garrett TPE 331-5 turbines 750 SHP 
