DOUGLAS DC-3

Basler BT-67
REFERENCE SHEET
For detailed instructions on how to fly this aircraft, see
Basler_BT67\Documentation\Flying the BT-67 in FSX.pdf

Total Flight Simulator aircraft weight with full fuel in main tanks Caution: Reduce load when using wing tip tanks | 28,746 lbs
Maximum Take-off Weight (MTOW) | 28,500
Maximum Landing Weight (MLW) | 27,300

Maximum Placard Speeds

VS - Stalling Speed clean | 68 KIAS
VSO - Stalling Speed in Landing Configuration | 62 KIAS
VNE – Never Exceed Speed | 228 KIAS
VNO - Turbulent Air Penetration Speed | 180 KIAS
VMC - Minimum Controllable Speed | 89 KIAS
VLE - Maximum Landing Gear Extension Speed | 166 KIAS
VY - Best Rate-of-Climb Speed (sea level) | 130 KIAS
VYSE - Single-engine Best Rate-of-Climb Speed | 120 KIAS

Maximum Flap Placard Speeds

Flaps | KIAS
1/4 | 133
1/2 | 99
Full | 97

V1 - Takeoff Decision Speed dry runway
Standard temperature, sea level pressure altitude

27,750 | 75 KIAS

VR - Rotation Speed dry runway
Standard temperature, sea level pressure altitude

27,750 | 87 KIAS

V2 - Minimum Climb Speed dry runway
Standard temperature, sea level pressure altitude

27,750 | 100 KIAS

Cruise Climb

Sea level to 10,000

## 135 KIAS

10,000 to 15,000 | 130 KIAS

VREF - Landing Approach Speed flaps down; gear down

20,000 lbs

## 75 KIAS

25,000 lbs | 80 KIAS