Basler BT-67

Basler BT-67 Checklist

COCKPIT |
Flight controls | free
Electrical switches | OFF
Avionics | OFF
Gear handle | DOWN
Parking brake | SET
Battery master | ON
Flaps | Test – extend to 1/4
Annunciator | checked
Fuel quantity | checked
Gear lights | Two ON
Battery master | OFF
Airplane papers | checked
Oxygen pressure | checked
Oxygen masks | checked
Oxygen control | OFF
BEFORE STARTING ENGINE |
Doors | closed and secure
Baggage | secure
Passenger briefing | completed
Seats | adjusted
Belts and harness | secure
Parking brake | SET
Fuel Cross feed | OFF
Firewall shut-off valves | ON
Power levers | IDLE
Prop controls | MAX RPM
Condition levers | STOP
Bleed air switches | ON
Electrical switches | OFF
Avionics master | OFF
Inverter power | OFF
Battery master | ON
Cockpit lights | check
Seat belts and No Smoking signs | ON
Navigation Lights | ON
Beacon | ON
Fuel quantity | checked
Trim | Set for Take-off
ENGINE START |
Battery (24-28V) | checked
Fuel pump
Fuel pressure | checked
Ignition switch | MANUAL
Starter | ON
Ng (min. 12%) | stabilized
Condition lever | RUN
Ignition light | ON
ITT (max. 1090°C for 2 sec.) and Ng | monitor
Ignition | AUTO
Generator | ON
Oil pressure | checked
Generator (when ammeter at 100 or less) | OFF
Both generators | ON
BEFORE TAXI |
Generators | ON
Bleed air switches | ON
APU | OFF
Lights | as required
Cabin comfort | as desired
Inverter power | ON
Generators | ON
Gyros | SET
Altimeter and clock | SET
Avionics master switch | ON
Autopilot | checked & OFF
Radios | checked
TAXIING |
Brakes | check
Flaps | 1/4
Flight instruments | Check
Power levers | IDLE
Prop control | FULL FORWARD
Condition levers | as required
Brakes | Check
Flaps | SET for TO
BEFORE TAKEOFF |
Fuel pumps | ON
Fuel pressure | Checked
Ice protection | as required
Flight instruments | Checked
Engine gauges | Checked
Warning lights | Checked
Radios and autopilot | SET
Prop sync | OFF
Trim | SET
Flaps | check and SET 1/4
Fuel quantity | Checked
Flight controls | Free
Fire wall shut-off valves | check - ON
TAKEOFF |
Directional gyro | runway heading
Power levers | Advance
Torque and ITT | within limits
Climb power | SET
Seat belts and no smoking signs | as required
Prop sync | as desired
Yaw damper | as desired
CRUISE |
Cruise power | SET
Engine instruments | check
Pressurization | as desired
Windshield heat | as required
BEFORE LANDING |
Seat belts and smoking lights | ON
Prop sync | OFF
Prop controls | 1700 RPM
Gear | down / 2 greens
Landing lights | ON
Autopilot/Yaw damper | OFF
BALKED LANDING |
Power | as required
Torque and temperatures | within limits
Airspeed | 70 kts
Flaps | 1/4
Gear | retracted
Airspeed | 90 kts
Flaps | UP
AFTER LANDING
Prop controls | MAX RPM
Reverse thrust (above 40 KIAS) | as desired
After clearing runway: |
Flaps | UP
Strobes | OFF
Trim | Neutral
SHUTDOWN
Parking brake | SET
Avionics | OFF
Electrical equipment | OFF
Inverter power | OFF
Battery charge | Checked
ITT below 610°C | one min.
Power lever | IDLE
Prop control | FEATHERED
Generator | OFF
Condition lever | STOP
Fuel pump (when 0% Ng) | OFF
Master comfort | OFF
Battery master | OFF