pc12.main_inst

Below we will run through the main instruments on the Pilatus PC12 panel. Most instruments are explained in greater detail and may be selected from the navigation bar. For a complete listing of all instruments on the main panel, please view below picture.

Avionics (Bendix/King)
• | 1 KMA26 Audio Control/Voice Activated Intercom with integrated Marker Beacon
• | 2 KX165A VHF COMM/NAV Transceivers
• | 1 KT70A ATC Transponder
• | 1 KEA 346 Encoding Altimeter
• | 1 KN63 DME
• | 1 KR87A Digital ADF System
• | KNI 582 RMI
• | EFS 40/50 Electronic Flight System:
|  | 2 ED462 EAS Tube EADI/EHSI 1 SG 465 EFIS Symbol Generator 1 CP 468 EFIS Control Panel
• | KFC325 Autopilot System:

KDC220 A/P Comp.
KDC222 Air Data Comp.
KTA33C Pitch Trim Adapter
3 KSA372 Servo
1 KAS 297C Altitude Pre-Selector
1 KMC 321 Mode Controller

• | 1 Litef AHRS - LCR92 - (Not Implemented in this panel)
• | 1 Narco ELT-910 Emergency Locator Transmitter - (Not Implemented in this panel)
Pilot Flight Instruments
• | 1 Airspeed Indicator
• | 1 Vertical Speed Indicator
• | 1 Clock/Stopwatch - (Combo GMT/LMT/Rate Indicator on EIS Display Unit)
• | 1 Standby Magnetic Compass
• | 1 Standby Attitude Indicator
• | 1 Standby Altimeter
Engine & Secondary Instruments
• | Torque Indicator
• | Turbine Temperature Indicator
• | Gas Generator Speed Indicator
• | Oil Temperature Indicator
• | Oil Pressure Indicator
• | Fuel Quantity Indicators (dual)
• | Fuel Flow Indicator
• | Fuel Used Indicator
• | Electrical Volts Indicator
• | Electrical Amps Indicator
• | Propeller Speed Indicator
• | OAT Indicator
Miscellaneous Instruments
• | 1 Flap Position Indicator
• | 1 Triple Trim Indicator - (Digital readout on lower left of EIS Display Unit)
• | 1 Cabin Rate of Climb Indicator - (Not Implemented in this panel)
• | 1 Cabin Altitude and Differential Pressure Indicator - (Not Implemented in this panel)
• | 3 Landing Gear Position Lights
• | 1 Oxygen Quantity Indicator - (Not Implemented in this panel)
• | 1 Flight Hour Recorder - (Not Implemented in this panel)